Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring IPv6 RIPng

Follow these steps to configure IPv6 RIPng on each switch:

1. Enable IPv6 unicast routing globally.

2. Enable IPv6 RIPng routing globally.

3. Enable RIPng routing on the desired interfaces.

- Enable RIPng

- Enable and Configure RIPng on Desired IPv6 Interfaces

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |