Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Create an RP-Set Table

1. In router A, associate the `VLAN 7` interface with PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# exit

2. Enter PIMv6 component mode for component 1.

       SEFOS(config)# ip pim component 1

3. Set the RP-candidate hold time to 30 seconds for PIMv6 component 1.

       SEFOS(pim-comp)# rp-candidate holdtime 30

4. Set the RP-candidate RP address (`7777::11`) for the group (`ff02::e001:1`) with a mask length of 128 in PIMv6 component 1.

       SEFOS(pim-comp)# ipv6 pim rp-candidate rp-address ff02::e001:1 128 7777::11
       SEFOS(pim-comp)# exit

5. Enter the interface configuration mode for `VLAN 7`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# shutdown

6. Set the BSR-candidate preference to 20 for the `VLAN 7` interface.

       SEFOS(config-if)# ipv6 pim bsr-candidate 20
       SEFOS(config-if)# exit

7. In router B, associate the `VLAN 7` interface with PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# exit

8. Enter PIMv6 component mode for component 1.

       SEFOS(config)# ip pim component 1

9. Set the RP-candidate hold time to 30 seconds for PIMv6 component 1.

       SEFOS(pim-comp)# rp-candidate holdtime 30
       SEFOS(pim-comp)# end

10. Set the RP-candidate address (`7777::11`) for the group (`ff02::e001:1`) with a mask length of 128 in PIMv6 component 1.

        SEFOS(pim-comp)# ipv6 pim rp-candidate rp-address ff02::e001:1 128 7777::21
        SEFOS(pim-comp)# exit

11. In router A, review the RP-set table.

        SEFOS# show ipv6 pim rp-set

        PIM Group-to-RP mappings
        ------------------------
        Group Address : ff02::e001:1Group Mask : 128
          RP: 7777::11
          Component-Id : 1
            Hold Time : 100, Expiry Time : 00:01:17

        Group Address : ff02::e001:1Group Mask : 128
          RP: 7777::21
          Component-Id : 1
            Hold Time : 110, Expiry Time : 00:01:37

12. In router B, review the RP-set table.

        SEFOS# show ipv6 pim rp-set 7777::11

        PIM Group-to-RP mappings
        ------------------------
          Group Address : ff02::e001:1Group Mask : 128
            RP: 7777::11
            Component-Id : 1
            Hold Time : 30, Expiry Time : 00:01:08

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |