Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

### Clearing the Snooping Statistics

The snooping statistics are updated for each VLAN whenever the various multicast packets are transmitted or received. The statistics are cleared per VLAN or for all VLANs based on the configuration. Before you can configure IGS features, you must configure your network environment, as described in Topology Example.

- Clear the Statistics for a Specific VLAN

- Clear the Statistics for All VLANs

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |