Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

## Configuring the VLAN Module

To make the PVRST+ module completely operational, you must configure the VLAN module. Before you configure VLAN as described in these sections, see VLAN Module to ensure that the configuration guidelines are satisfied.

The examples in this section use switch B (hostname TOR-1), port 0/1, and `VLAN 10` and `VLAN 20`.

- Disable GVRP

- Configuring Trunk and Access Ports

- Configure VLANS and Display the PVRST+ Information for VLANs

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |