Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Settings

The following table contains the default settings that are configured for PIM in a SEFOS switch. If the switch is rebooted for any reason, it returns to the previously saved configuration. If you have not saved a site configuration, the reboot returns the switch to the default settings. For instructions on how to save your site configuration, refer to the software configuration guide for your switch.

Feature | Default Setting
--- | ---
PIM module status | Enabled
PIM SPT group threshold | 0
PIM SPT source threshold | 0
PIM SPT-switch period | 0 seconds
PIM RP-threshold | 0
PIM RP-switch period | 0 second
PIM regstop-ratelimit-period | 5 seconds
PIM PMBR status | disable
PIM static-RP | disable
PIM component mode | sparse
RP-candidate holdtime | 0 second
PIM query-interval | 30 seconds
PIM message-interval | 60 seconds
PIM bsr-candidate | 0
PIM component ID | 1
PIM hello-hold time | 105 seconds
PIM DR-priority | 1
PIM override-interval | 0 second
PIM lan-delay | 0 second
PIM lan-prune-delay | disable

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |