Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Report Forwarding

By default, an IGMP report message is forwarded on all of the router ports in a VLAN. However, you can configure the reports to be forwarded on the member ports of the VLAN. Before you can configure IGS features, you must configure your network environment, as described in Topology Example.

- Enable Report Forwarding

- Disable Report Forwarding

- Reset Report Forwarding to the Default Value

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |