C H A P T E R 13

XVLAN

Ports in XVLAN can be classified into three types: internal, external and inter-switch trunk ports. XVLANs require that the ports assigned to internal, external and inter-switch trunk, be mutually exclusive and should not overlap. If the port lists overlap, then the XVLAN will be misconfigured and may not function correctly. Similarly, it is required that the port lists across multiple Principal Exclusive VLANs be mutually exclusive and should not overlap.

An XVLAN consists of two types of XVLANs: principal and restricted exclusive VLANs.

##

13.1 Principal XVLAN

Principal XVLAN is in fact the actual VLAN, providing communication with network devices outside the XVLAN domain. In effect, it is the main VLAN and is used to carry the XVLAN’s traffic upstream to the outside world.

The maximum number of principal XVLANs supported on the switch is 12.

##

13.2 Restricted XVLANs

There are two types of restricted XVLANs. The main difference between the two types is whether the ports within the restricted XVLAN can communicate to each other or not.

The maximum number of restricted XVLANs configurable under a principal XVLAN is 15.

### 13.2.1 Solitary (Solo) Restricted XVLAN

This type of XVLAN provides isolation between the ports within the restricted XVLAN. Ports in the solitary restricted XVLAN can not communicate with each other. In order to communicate with devices outside the XVLAN, frames have to go over the principal XVLAN’s external ports. Since this type of XVLAN provides isolation within it’s member ports, a single Solitary XVLAN is sufficient for a given XVLAN domain.

### 13.2.2 Group Restricted XVLAN

Group Restricted XVLAN allows communication between its member ports. Isolation between multiple group or solitary restricted XVLANs is maintained. Communication to devices outside the XVLAN domain has to go through the external ports of the principal XVLAN. There could be multiple restricted group XVLANs in a given XVLAN.

The maximum number of restricted XVLANs configurable under a principal XVLAN is 15.

##

13.3 Port Types in XVLANs

Ports in XVLAN can be classified into three types.

### 13.3.1 External Ports

These ports are used to communicate to the outside world. Frames enter and leave the XVLAN through these ports. Devices like routers and shared resources could be connected to these ports.

### 13.3.2 Internal Ports

These ports are used to connect to the hosts on the restricted XVLANs.

### 13.3.3 Inter-Switch Trunk Ports

These ports are a generic trunk (or hybrid) ports, used to interconnect multiple switches that belong to the same XVLAN. The isolation behavior of the restricted XVLANs is extended and maintained on all the switches belonging to the same XVLAN domain. Inter-Switch Trunk ports can be shared with regular VLANs.

##

13.4 Config Modes and CLI Commands

The list of CLI commands for the configuration of XVLANs is as follows:

- Global Config Mode

- `xvlan vid`

- `no xvlan vid`

- XVLAN Config Mode

- ports `internal IFLIST external IFLIST inter-switch-trunk IFLIST name`

- ports add `internal IFLIST external IFLIST inter-switch-trunk IFLIST name`

- `no ports internal IFLIST external IFLIST inter-switch-trunk IFLIST name`

- xvlan vid `type ports internal IFLIST external IFLIST inter-switch-trunk IFLIST name`

- `no` xvlan vid

- `xvlan vid type ports add internal IFLIST external IFLIST inter-switch-trunk IFLIST name`

- `xvlan vid type no ports internal IFLIST external IFLIST inter-switch-trunk IFLIST name`

- switchport xvlan-vlan-shared

- `no` switchport xvlan-vlan-shared

- Privileged EXEC Mode

- show xvlan

- show xvlan `summary`

- `show xvlan vid`

##

13.5 XVLAN Commands

The list of XVLAN commands is as follows:

- xvlan vid

- ports

- ports add

- xvlan vid type ports

- switchport xvlan-vlan-shared

- `no` switchport xvlan-vlan-shared

- show xvlan

- show running-config

- show vlan port config port

### 13.5.1 `xvlan vid`

Creates a principal XVLAN and changes the configuration mode to XVLAN configuration mode. GVRP must be disabled before running this command. The `no` form of the command deletes the XVLAN.

    xvlan 2-4094

    no xvlan 2-4094

Mode | Global Configuration
Example | SEFOS(config)# xvlan 10 SEFOS(config-xvlan)# SEFOS(config)# no xvlan 10
Notes | GVMRP must be disabled.

### 13.5.2 `ports`

Configures ports for the principal XVLAN. Ports are designated as internal, external, and inter-switch trunks. The resulting port pool is used by the restricted XVLANs. The `no` form of the command resets the port list or the subset for the specified XVLAN.

    ports (internal [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) (external [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) (inter-switch [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) [name vlan-name]

    no ports (internal [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) (external [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) (inter-switch [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) [name vlan-name]

Syntax Description | internal interface-type 0/a-b,0/c,...- Internal and restricted ports interface type and identifier. external interface-type 0/a-b,0/c,... - External ports interface type and identifier. port-channel a,b,c-d - Port-channel identifier. inter-switch - Inter switch trunk ports interface type and identifier name - XVLAN identifier name string.
Mode | XVLAN Configuration
Example | SEFOS(config-xvlan)# ports internal ext 0/2,0/11,0/15 external ext 0/1 inter-switch port-channel 36,710 SEFOS(config-xvlan)# SEFOS(config-xvlan)# no ports internal ext 0/15

#### Related Commands

- xvlan vid - Create principal XVLAN

- ports add - Add ports to existing principal XVLAN port membership port list

- `no` ports - Remove ports from an existing XVLAN port membership port list

- xvlan vid type ports - Create a restricted XVLAN and assign port membership from the principal XVLAN’s port list pool

### 13.5.3 `ports add`

Adds ports for the existing principal XVLAN port list.

    ports add (internal [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) (external [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) (inter-switch [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) [name vlan-name]

Syntax Description | internal interface-type 0/a-b,0/c,...- Internal and restricted ports interface type and identifier. external interface-type 0/a-b,0/c,... - External ports interface type and identifier. port-channel a,b,c-d - Port-channel identifier. inter-switch - Inter switch trunk ports interface type and identifier. name - XVLAN identifier name string.
Mode | XVLAN Configuration
Example | SEFOS(config-xvlan)# ports add internal ext 0/19 SEFOS(config-xvlan)#
Notes | XVLANs require that the ports assigned to internal, external, and inter-switch trunk, be mutually exclusive. If this mutual exclusion requirement is not followed, the XVLAN will be misconfigured and it may not function correctly.

#### Related Commands

- xvlan vid - Create principal XVLAN

- ports - Assign ports to principal XVLAN port membership port list

- `no` ports - Remove ports from an existing XVLAN port membership port list

- xvlan vid type ports - Create a restricted XVLAN and assign port membership from the principal XVLAN’s port list pool

### 13.5.4 `xvlan vid type ports`

Creates a restricted XVLAN and assigns port membership to it. The ports are used from the pool assigned to the principal XVLAN. The type of the restricted XVLAN must be specified as well.

Note - The `vid` of the restricted XVLAN must be higher than the `vid` of the principal XVLAN.

    xvlan vid type ports (internal [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) (external [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d] [all]) (inter-switch-trunk [interface-type 0/a-b,0/c,...] [interface-type 0/a-b,0/c,...] [port-channel a,b,c-d]) [name vlan-name]

Syntax Description | vid - Restricted XVLAN identifier. type - Restricted XVLAN type: `solo`: Restricted solitary. `group`: Restricted group. port - Ports key word. internal interface-type 0/a-b,0/c,...- Internal and restricted ports interface type and identifier. external interface-type 0/a-b,0/c,... - External ports interface type and identifier. port-channel a,b,c-d - Port-channel identifier. inter-switch - Inter switch trunk ports interface type and identifier name - XVLAN identifier name string.
Mode | XVLAN Configuration
Example | SEFOS(config-xvlan)# xvlan 100 solo ports internal ext 0/2,0/11,0/15 external ext 0/1 inter-switch port-channel 36,710 SEFOS(config-xvlan)#
Notes | The `vid` of the restricted XVLAN must be higher than the `vid` of the principal XVLAN. XVLANs require that the ports assigned to internal, external and inter-switch trunk, be mutually exclusive. If this mutual exclusion requirement is not followed, the XVLAN will be misconfigured and it may not function correctly.

#### Related Commands

- xvlan vid - Create Principal XVLAN

- ports add - Add Ports to existing principal XVLAN port membership port list

- `no` ports - Remove ports from an existing XVLAN port membership port list

- xvlan vid type ports - Create a restricted XVLAN and assign port membership from the principal XVLAN’s port list pool

### 13.5.5 `switchport xvlan-vlan-shared`

Allows the configuration of regular VLANs on an internal port of an exclusive VLAN. The `no` form of the command disables this feature...

    switchport xvlan-vlan-shared

    no switchport xvlan-vlan-shared

Mode | Interface Configuration
Defaults | Disabled.
Example | SEFOS(config-if)# switchport xvlan-vlan-shared
Notes | When `xvlan-vlan-shared` mode is disabled (default), the port can be configured as a member of either a regular or exclusive VLAN. However, the port can not be shared. When `xvlan-vlan-shared` mode is enabled and the port is configured as an internal port of an exclusive VLAN, the port can be configured as a tagged member of a regular VLAN. However, the port can not be configured as an untagged member of the regular VLAN. The `xvlan-vlan-shared` command is effective only if the port is in XVLAN mode. Thus, the configuration procedure for XVLAN/VLAN port sharing is as follows: 1. Configure XVLAN. 2. Set `xvlan-vlan-shared` mode for the ports of interest. 3. Configure regular VLAN.

#### Related Commands

- show vlan port config port - Displays the VLAN related parameters specific for ports

- show running-config - Displays the current configuration

- ports add - Add Ports to existing principal XVLAN port membership port list

- `no` ports - Remove ports from an existing XVLAN port membership port list

- xvlan vid type ports - Create a restricted XVLAN and assign port membership from the principal XVLAN’s port list pool

### 13.5.6 `show xvlan`

Displays XVLAN database.

    show xvlan  [vid vlan-range | summary]

Syntax Description | xvlan - XVLAN interface
Mode | Privileged EXEC
Example | SEFOS# show xvlan Exclusive Vlan database --------------------------- XVlan ID : 100 Type : Restricted: Group Principal XVlan : 10 External Ports : Ex0/1 Internal Ports : Ex0/11 ISWTrunk Ports : po36, po710 Name : ---------------------------------------------------- XVlan ID : 20 Type : Restricted: Group Principal XVlan : 10 External Ports : Ex0/1 Internal Ports : Ex0/15 ISWTrunk Ports : po36, po710 Name -------------------------- XVlan ID : 10 Type : Principal Principal XVlan : 10 External Ports : Ex0/1 Internal Ports : Ex0/2, Ex0/11, Ex0/15, Ex0/19 ISWTrunk Ports : po36, po710 Name : main ----------------------------------------------------
| XVlan ID : 600 Type : Restricted: Solitary Principal XVlan : 10 External Ports : Ex0/1 Internal Ports : Ex0/2 ISWTrunk Ports : po36, po710 Name : sub1 SEFOS# show xvlan summary Exclusive VLAN 10 Summary ------------------------------- XVLAN ID Type ------------------------------- 10: Principal 600: Restricted: Solitary 100: Restricted: Group 20: Restricted: Group ---------------------------------------------------- SEFOS# show xvlan vid 10 Exclusive Vlan database --------------------------- XVlan ID : 10 Type : Principal Principal XVlan : 10 External Ports : Ex0/1 Internal Ports : Ex0/2, Ex0/11, Ex0/15, Ex0/19 ISWTrunk Ports : po36, po710 Name : main

#### Related Commands

- xvlan vid type ports - Create restricted XVLAN and assign port membership

- xvlan vid - Create principal XVLAN and change to XVLAN configuration mode

- `no` xvlan vid - Delete the principal XVLAN with `vid`

- ports add - Add ports to existing principal XVLAN port membership port list

- `no` ports - Remove ports from an existing XVLAN port membership port list

### 13.5.7 `show running-config`

Displays the current running VLAN and XVLAN configuration.

    show running-config vlan

Syntax Description | vlan - XVLAN interface
Mode | Privileged EXEC
Example | SEFOS# show running-config vlan Building configuration... ! ! xvlan 10 port internal extreme-ethernet 0/2,0/11,0/15,0/19 external extreme-ethernet 0/1 inter-switch port-channel 36,710 name main xvlan 600 solo port internal extreme-ethernet 0/2 external extreme-ethernet 0/1 inter-switch port-channel 36,710 name sub1 xvlan 100 group port internal extreme-ethernet 0/11,0/19 external extreme-ethernet 0/1 inter-switch port-channel 36,710 xvlan 20 group port internal extreme-ethernet 0/15 external extreme-ethernet 0/1 inter-switch port-channel 36,710 ! ?...

#### Related Commands

- xvlan vid type ports - Create restricted XVLAN and assign port membership

- xvlan vid - Create principal XVLAN and change to XVLAN configuration mode

- `no` xvlan vid - Delete the principal XVLAN with `vid`

- ports add - Add ports to existing principal XVLAN port membership port list

- `no` ports - Remove ports from an existing XVLAN port membership port list

- show vlan - Show VLAN port membership

- show xvlan - XVLAN port membership

- show vlan port config - Show VLAN related port properties

### 13.5.8 `show vlan port config port`

Displays the VLAN properties for a given port.

    show vlan port config [{port interface-type interface-id | switch switch-or-context-name}]

Syntax Description | vlan - XVLAN interface
Mode | Privileged EXEC
Example | SEFOS# show vlan port config Vlan Port configuration table ------------------------------- Port Ex0/1 Port Vlan ID : 10 Port Acceptable Frame Type : Admit All Port Ingress Filtering : Enabled Port Mode : Hybrid Exclusive VLAN Port Mode : External VLAN & Exclusive VLAN Port Sharing : Enabled Exclusive VLAN VID : 10 Port Gvrp Status : Enabled Port Gmrp Status : Enabled Port Gvrp Failed Registrations : 0 Gvrp last pdu origin : 00:00:00:00:00:00 Port Restricted Vlan Registration : Disabled Port Restricted Group Registration : Disabled Mac Based Support : Disabled Subnet Based Support : Disabled Port-and-Protocol Based Support : Enabled
| Default Priority : 0 Dot1x Protocol Tunnel Status : Peer LACP Protocol Tunnel Status : Peer Spanning Tree Tunnel Status : Peer GVRP Protocol Tunnel Status : Peer GMRP Protocol Tunnel Status : Peer IGMP Protocol Tunnel Status : Peer Filtering Utility Criteria : Default Port Protected Status : Disabled ------------------------------------------------------- Port Ex0/2 Port Vlan ID : 600
| Port Acceptable Frame Type : Admit All Port Ingress Filtering : Disabled Port Mode : Hybrid Exclusive VLAN Port Mode : Internal Exclusive VLAN VID : 600 Port Gvrp Status : Enabled Port Gmrp Status : Enabled Port Gvrp Failed Registrations : 0 Gvrp last pdu origin : 00:00:00:00:00:00 Port Restricted Vlan Registration : Disabled Port Restricted Group Registration : Disabled Mac Based Support : Disabled Subnet Based Support : Disabled
| Port-and-Protocol Based Support : Enabled Default Priority : 0 Dot1x Protocol Tunnel Status : Peer LACP Protocol Tunnel Status : Peer Spanning Tree Tunnel Status : Peer GVRP Protocol Tunnel Status : Peer GMRP Protocol Tunnel Status : Peer IGMP Protocol Tunnel Status : Peer Filtering Utility Criteria : Default Port Protected Status : Disabled ---------------------------------------------------

The following example shows detailed port information for the given VLAN and XVLAN and configuration. In the example, ports Ex0/1, Ex0/2, Ex0/11, Ex0/15, Ex0/19, port-channel 36, and port-channel 710 belong to principal XVLAN 10 and its restricted XVLANs 20, 100 and 600. Whereas, the rest belong to the default VLAN 1.

    SEFOS# show xvlan

    Exclusive Vlan database
    ---------------------------

    XVlan ID            : 10
    Type                : Principal
    Principal XVlan     : 10
    External Ports      : Ex0/1
    Internal Ports      : Ex0/2, Ex0/11, Ex0/15, Ex0/19
    ISWTrunk Ports      : po36, po710

    Name                : main
    ----------------------------------------------------
    XVlan ID            : 20
    Type                : Restricted: Group
    Principal XVlan     : 10
    External Ports      : Ex0/1
    Internal Ports      : Ex0/15
    ISWTrunk Ports      : po36, po710
    Name                :
    ----------------------------------------------------

    XVlan ID            : 100
    Type                : Restricted: Group
    Principal XVlan     : 10
    External Ports      : Ex0/1
    Internal Ports      : Ex0/11, Ex0/19
    ISWTrunk Ports      : po36, po710
    Name                :
    ----------------------------------------------------
    XVlan ID            : 600
    Type                : Restricted: Solitary
    Principal XVlan     : 10
    External Ports      : Ex0/1
    Internal Ports      : Ex0/2
    ISWTrunk Ports      : po36, po710
    Name                : sub1
    ----------------------------------------------------
    SEFOS# show vlan port config

    Vlan Port configuration table
    -------------------------------
    Port Ex0/1
     Port Vlan ID                        : 10
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Exclusive VLAN Port Mode            : External
     Exclusive VLAN VID                  : 10
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/2
     Port Vlan ID                        : 600
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
    Port Mode                           : Hybrid
     Exclusive VLAN Port Mode            : Internal
     Exclusive VLAN VID                  : 600
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled

      Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/11
     Port Vlan ID                        : 100
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Exclusive VLAN Port Mode            : Internal
     Exclusive VLAN VID                  : 100
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    ?......
     -------------------------------------------------------
    Port Ex0/14
     Port Vlan ID                        : 1
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/15
     Port Vlan ID                        : 20
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Exclusive VLAN Port Mode            : Internal
     Exclusive VLAN VID                  : 20
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/16
     Port Vlan ID                        : 1
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
    GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/17
     Port Vlan ID                        : 1
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/18
     Port Vlan ID                        : 1
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/19
     Port Vlan ID                        : 100
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Exclusive VLAN Port Mode            : Internal
     Exclusive VLAN VID                  : 100
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port Ex0/20
     Port Vlan ID                        : 1
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    ?.....
     -------------------------------------------------------
    Port po36
     Port Vlan ID                        : 10
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Exclusive VLAN Port Mode            : Inter-Switch Trunk
     Exclusive VLAN VID                  : 10
     Port Gvrp Status                    : Enabled
     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled
     -------------------------------------------------------
    Port po710
     Port Vlan ID                        : 10
     Port Acceptable Frame Type          : Admit All
     Port Ingress Filtering              : Disabled
     Port Mode                           : Hybrid
     Exclusive VLAN Port Mode            : Inter-Switch Trunk
     Exclusive VLAN VID                  : 10
     Port Gvrp Status                    : Enabled

     Port Gmrp Status                    : Enabled
     Port Gvrp Failed Registrations      : 0
     Gvrp last pdu origin                : 00:00:00:00:00:00
     Port Restricted Vlan Registration   : Disabled
     Port Restricted Group Registration  : Disabled
     Mac Based Support                   : Disabled
     Subnet Based Support                : Disabled
     Port-and-Protocol Based Support     : Enabled
     Default Priority                    : 0
     Dot1x Protocol Tunnel Status        : Peer
     LACP Protocol Tunnel Status         : Peer
     Spanning Tree Tunnel Status         : Peer
     GVRP Protocol Tunnel Status         : Peer
     GMRP Protocol Tunnel Status         : Peer
     IGMP Protocol Tunnel Status         : Peer
     Filtering Utility Criteria          : Default
     Port Protected Status               : Disabled

#### Related Commands

- xvlan vid type ports - Create restricted XVLAN and assign port membership

- xvlan vid - Create principal XVLAN and change to XVLAN configuration mode

- `no` xvlan vid - Delete the principal XVLAN with `vid`

- ports add - Add ports to existing principal XVLAN port membership port list

- `no` ports - Remove ports from an existing XVLAN port membership port list

- show xvlan - XVLAN port membership

- show vlan port config - Show VLAN related port properties

Copyright © 2012, Oracle and/or its affiliates. All rights reserved.