Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring OSPFv3 Interface Parameters

All of the OSPF interface sample configurations in this section are executed in SEFOS1. See IPv6 Example Topology Interface and Host Addresses for the topology used for the configuration of the parameters in this section.

- OSPFv3 Interface Parameters

- Configure Interface Priority

- Restore the Default Interface Priority

- Configure the Retransmission Interval

- Restore the Default Retransmission Value

- Configure Transmission Delay

- Restore the Default Transmission Delay

- Configure the Hello Interval

- Restore the Default Hello Interval

- Configure the Dead Interval

- Restore the Default Dead Interval

- Configure the Network Type

- Restore the Default OSPF Network Type

- Configure the Interface Cost

- Restore the Default Interface Cost

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |