Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Multicast Router Ports

Multicast router ports for a VLAN can be configured statically or learned dynamically. When a port receives a query message, that port is added to the multicast router port list.

When configuring multicast router ports for a VLAN, you can specify the amount of time after which dynamically learned router entries will be deleted. You can also configure a switch to function as a querier on a particular VLAN, and you can specify the amount of time a switch will wait to determine if hosts are still interested in a specific multicast group.

- Configure a Static Multicast Router Port

- Delete Configured Router Ports

- Configure Dynamically Learned Multicast Router Port Time-Out

- Restore the Port-Purge Interval

- Configure an MLDS Switch as a Querier

- Configure MLDS Query Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |