Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS2

Configure `VLAN 10` and `VLAN 40` interfaces on SEFOS2 in the example topology.

1. Configure SEFOS2.

       SEFOS 2 SEFOS# configure terminal
       SEFOS 2 SEFOS(config)# set gvrp disable
       SEFOS 2 SEFOS(config)# set gmrp disable

       SEFOS 2 SEFOS(config)# interface extreme-ethernet 0/15
       SEFOS 2 SEFOS(config-if)# switchport access vlan 10
       % Access VLAN does not exist.,Creating vlan
       SEFOS 2 SEFOS(config-if)# exit

       SEFOS 2 SEFOS(config)# interface vlan 10
       SEFOS 2 SEFOS(config-if)# no shut
       SEFOS 2 SEFOS(config-if)# ipv6 enable
       SEFOS 2 SEFOS(config-if)# ipv6 address 1111::12 112
       SEFOS 2 SEFOS(config-if)# exit

       SEFOS 2 SEFOS(config)# interface vlan 40
       SEFOS 2 SEFOS(config-if)# no shut
       SEFOS 2 SEFOS(config-if)# ipv6 enable
       SEFOS 2 SEFOS(config-if)# ipv6 address 4444::12 112
       SEFOS 2 SEFOS(config-if)# exit

       SEFOS 2 SEFOS(config)# vlan 40
       SEFOS 2 SEFOS(config-vlan)# ports extreme-ethernet 0/3
       SEFOS 2 SEFOS(config-vlan)# exit

       SEFOS 2 SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS 2 SEFOS(config-if)# no shut
       SEFOS 2 SEFOS(config-if)# end

2. Show the status of IPv6 interfaces on SEFOS2.

       SEFOS 2 SEFOS# show ipv6 interface
       vlan1 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:630f
           Global unicast address(es):
               Not Configured.
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff6c:630f
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan40 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:630f
           Global unicast address(es):
               4444::12/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::9
               ff02::1:ff00:12
               ff02::1:ff6c:630f
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan10 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::214:4fff:fe6c:630f
           Global unicast address(es):
               1111::12/112
               6666::12/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::9
               ff02::1:ff00:12
               ff02::1:ff6c:630f
           MTU is 9216
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |