Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Trunk and Access Ports

After you enable the PVRST+ software, you must explicitly use commands to configure ports as trunk or access, in order to make them a member of a VLAN. After you configure the port as a trunk port, it becomes a member port of all active VLANs in the system. After you configure a port as access, the port becomes a member port of the VLAN that is configured as PVID for that port.

- Configure a Trunk Port

- Configure an Access Port

- Set Up PVID on a Port

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |