Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure LLDP Global Objects

Global objects are system-specific objects that are common for all interfaces in the system.

1. At switch 1, change the global configuration of LLDP.

       SEFOS# configure terminal
       SEFOS(config)# lldp transmit-interval 15
       SEFOS(config)# lldp holdtime-multiplier 2
       SEFOS(config)# lldp reinitialization-delay 5
       SEFOS(config)# lldp tx-delay 3
       SEFOS(config)# lldp notification-interval 10
       SEFOS(config)# lldp chassis-id-subtype local "switch"
       SEFOS(config)# end

   The values given to each parameter in this step are examples only.

2. Review the values of global configuration.

       SEFOS# show lldp
       LLDP is disabled
       Transmit Interval        : 15
       Holdtime Multiplier        : 2
       Reinitialization Delay    : 5
       Tx Delay            : 3
       Notification Interval    : 10
       Chassis Id SubType        : Local
       Chassis Id            : switch

3. Reset the LLDP global configuration to the default values.

       SEFOS# configure terminal
       SEFOS(config)# no lldp transmit-interval
       SEFOS(config)# no lldp holdtime-multiplier
       SEFOS(config)# no lldp reinitialization-delay
       SEFOS(config)# no lldp tx-delay
       SEFOS(config)# no lldp notification-interval
       SEFOS(config)# lldp chassis-id-subtype mac-addr
       SEFOS(config)# end

4. View the LLDP global configuration.

       SEFOS# show lldp
       LLDP is disabled
       Transmit Interval        : 30
       Holdtime Multiplier        : 4
       Reinitialization Delay    : 2
       Tx Delay            : 2
       Notification Interval    : 5

       Chassis Id SubType        : Mac Address
       Chassis Id            : 00:01:02:03:04:01

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |