Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable OSPF Over the VLAN Interface

Configure the interface parameters in Interface Configuration mode.

- Enable OSPF over the VLAN interface and associate the interface with an OSPF area before configuring OSPF interface parameters.

  VLAN interfaces `VLAN 1` and `VLAN 10` are created as part of the prerequisite configuration.

      SEFOS# configure terminal
      SEFOS(config)# router ospf
      SEFOS(config-router)# router-id 10.10.2.1
      SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
      SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6
      SEFOS(config-router)# exit
      SEFOS(config)# interface vlan 1
      SEFOS(config-if)#

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |