Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure PIMv6 in Router A

1. Enable IPv6, and configure the interface in `VLAN 7`.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# shutdown
       SEFOS(config-if)# ipv6 enable
       SEFOS(config-if)# ipv6 address 7777::11 112 unicast
       SEFOS(config-if)# ipv6 address fe80::7777:11 link-local
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit
       SEFOS(config)# int ext 0/3
       SEFOS(config-if)# switchport acce vlan 7

       % Access VLAN does not exist.,Creating vlan
       SEFOS(config-if)# no shut
       SEFOS(config-if)# exit

2. Enable IPv6, and configure the interface in `VLAN 2`.

       SEFOS(config)# interface vlan 2
       SEFOS(config-if)# shutdown
       SEFOS(config-if)# ipv6 enable
       SEFOS(config-if)# ipv6 address 2222::12 112 unicast
       SEFOS(config-if)# ipv6 address fe80::2222:12 link-local
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit
       SEFOS(config)# int extreme-ethernet 0/15
       SEFOS(config-if)# switchport access vlan 2

       % Access VLAN does not exist.,Creating vlan
       SEFOS(config-if)# no shut
       SEFOS(config-if)# exit

3. Add a static route by using the local address for the sender and listener.

       SEFOS(config)# ipv6 route 3333::0 112 fe80::7777:21 vlan 7
       SEFOS(config)# exit

4. Review the IPv6 output.

       SEFOS# show ipv6 interface

       vlan1 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::221:28ff:fe56:d7a9
           Global unicast address(es):
               Not Configured.
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff56:d7a9
           MTU is 1500
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan7 is up, line protocol is down
           IPv6 is Enabled
           Link local address:
               fe80::7777:11    [Down]
               fe80::221:28ff:fe56:d7a9    [Down]
           Global unicast address(es):
               7777::11/112    [Down]
           Joined group address(es):
               Not Configured.
           MTU is 1500
           ICMP redirects are enabled
           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled
       vlan2 is up, line protocol is up
           IPv6 is Enabled
           Link local address:
               fe80::2222:12
           Global unicast address(es):
               2222::12/112
           Joined group address(es):
               ff02::1
               ff02::2
               ff02::1:ff00:12
               ff02::1:ff22:12
           MTU is 1500
           ICMP redirects are enabled

           ND DAD is enabled, Number of DAD attempts: 1
           ND router advertisement is disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |