Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Examine the Configuration Details in SEFOS4

- Type.

      SEFOS# show ip ospf route

      OSPF Process Routing Table
      Dest/Mask                     TOS NextHop/Interface Cost Rt.Type   Area
      ---------                     --- -------/--------- ---- -------   ----SEFOS# show ip ospf 0.0.0.0 database external
      10.5.5.0/255.255.255.0        0   0.0.0.0/vlan4     1    IntraArea 0.0.0.0
      10.8.0.0/255.255.0.0          0   10.5.5.5/vlan4    2    InterArea 0.0.0.0OSPF Router with ID (10.4.0.4)                  AS External Link States                  -----------------------LS age                : 300Options               : (No ToS Capability, DC)LS Type              : AS External LinkLink State ID        : 10.4.0.0Advertising Router     : 10.4.0.4LS Seq Number         : 0x80000001Checksum             : 0x2a6Length               : 36Network Mask         : 255.255.0.0Metric Type          : 0x80Metric            : 10Forward Address      : 0.0.0.0Externel Route Tag    : 0                  AS External Link States                  -----------------------LS age             : 300Options            : (No ToS Capability, DC)LS Type            : AS External LinkLink State ID      : 10.5.5.0Advertising Router : 10.4.0.4LS Seq Number      : 0x80000001Checksum           : 0xbee3Length             : 36Network Mask       : 255.255.255.0Metric Type        : 0x80Metric             : 10Forward Address    : 0.0.0.0Externel Route Tag : 0
       AS External Link States
       -----------------------
      LS age             : 300AS External Link States                  -----------------------LS age             : 300Options            : (No ToS Capability, DC)LS Type            : AS External LinkLink State ID      : 100.0.0.0Advertising Router : 10.4.0.4LS Seq Number      : 0x80000001Checksum           : 0xcd6bLength             : 36Network Mask       : 255.0.0.0Metric Type        : 0x80Metric             : 10Forward Address    : 10.5.5.5Externel Route Tag : 0
      Options            : (No ToS Capability, DC)
      LS Type            : AS External Link
      Link State ID      : 10.5.6.0
      Advertising Router : 10.4.0.4
      LS Seq Number      : 0x80000001
      Checksum           : 0xb3ed
      Length             : 36
      Network Mask       : 255.255.255.0
      Metric Type        : 0x80
      Metric             : 10
      Forward Address    : 0.0.0.0
      Externel Route Tag : 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |