Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

#### RIPng Topology Example

The following illustration shows a a RIP topology in which the three switches are connected over multiple VLANs interfaces. Switch SEFOS1 has `VLAN 30`, `40`, and `50` configured. Switch SEFOS 3 has VLAN 20 and 30 configured, and switch 2 has `VLAN 40` and `VLAN 10` configured.

Before configuring the switch to run IPv6 RIPng protocol, IPv6 unicast-routing must be enabled globally, and IPv6 must be enabled on any interface on which IPv6 RIPng is to be processed. This guide describes how to configure RIPng for IPv6 in SEFOS switches and provides configuration examples on the topology shown below.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |