Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Fast Leave

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Enable fast leaving.

       SEFOS(config-if)# ip igmp immediate-leave
       SEFOS(config-if)# end

3. Ensure that fast leave is enabled on the interface.

       SEFOS# show ip igmp interface vlan 2

       ...
        Fast leave is enabled on this interface
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |