Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

#### Switch A

Switch A has the following specifications:

- Port 2 is connected to port 33 of a third-party DCBX-capable switch.

- Port 18 is connected to the host blade server.

- `VLAN 201` is assigned to port 2 and port 18.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |