Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Dynamically Learned Multicast Router Port Time-Out

Configuring the MLDS router purge time-out deletes the dynamically learned multicast router ports if no MLD router control packets are received. Use the `mrouter-time-out` command to set the aging-out time after multicast router ports are dynamically learned, as shown in the following example.

The default value for the multicast router port time-out is 125 seconds. This example configures the value as 60. Dynamically learned router entries will be deleted after 60 seconds.

1. Configure the multicast router port time-out value.

       SEFOS# configure terminal
       SEFOS(config)# ipv6 mld snooping mrouter-time-out 60
       SEFOS(config)# end

2. View the configuration.

       SEFOS# show ipv6 mld snooping globals

       Snooping Configuration
       -----------------------------
       MLD Snooping globally enabled
       MLD Snooping is operationally enabled
       Transmit Query on Topology Change globally disabled
       Multicast forwarding mode is MAC based
       Proxy globally disabled
       Proxy reporting globally enabled
       Filter is disabled
       Router port purge interval is 60 seconds
       Port purge interval is 260 seconds
       Report forward interval is 5 seconds
       Group specific query interval is 2 seconds
       Reports are forwarded on router ports
       Group specific query retry count is 2
       Multicast VLAN disabled

       Leave config level is Vlan based

   Note that statically configured router ports are not deleted after the router purge time interval.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |