Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Interval Between Generation of Configuration Messages

These topics describe how to configure the interval between generation of configuration messages.

- Configure the MST Interval Between Generation of Configuration Messages

- Restore the Default Interval Between Generation of Configuration Messages

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |