Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DCB Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable DCB for Each Interface

By default, all three features are enabled. However, to use the features, the global interface state must be turned on.

This example uses port 0/2.

1. Enable DCB on a specific interface.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/2
       SEFOS(config-if)# set dcb enable
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# end

2. View the interface configuration.

   These examples show the default configurations.

       SEFOS# show interfaces extreme-ethernet 0/2 description
       Interface    Status   Protocol
       ---------    ------   --------
       Ex0/2        up       up

3. Display the DCB state and feature mode on a specific interface.

       SEFOS# show interfaces extreme-ethernet 0/2 dcb mode

       Port                  : Ex0/2
       Show Type             : Admin State
       DCB Capable State     : on
       Priority Group        : auto
       Priority Flow Control : auto

4. Display the local configuration of the priority group.

       SEFOS# show interfaces extreme-ethernet 0/2 dcb priority-group

       Port             :      Ex0/2
       Show Type        :      Admin Config
       Feature          :      Priority Group
       Enable           :      true
       Advertise        :      true
       Willing          :      false
       Group Bandwidth  :      50%     30%     20%     0%      0%      0%      0%      0%
       Priority Group ID:      0       0       0       1       2       2       2       15
       Max Traffic Class:      8

5. Display the local configuration of the priority flow control feature.

       SEFOS# show interfaces extreme-ethernet 0/2 dcb priority-flow-control
       Port             :      Ex0/2
       Show Type        :      Admin Config
       Feature          :      Priority Flow Control
       Enable           :      true
       Advertise        :      true
       Willing          :      false
       Priority Mask    :      0       0       0       1       0       0       0       0
       Max Traffic Class:      8

6. Display the local configuration of the application feature.

       SEFOS# show interfaces extreme-ethernet 0/2 dcb application-etype-fcoe

       Port             :      Ex0/2
       Show Type        :      Admin Config
       Feature          :      Application FCoE
       Enable           :      true
       Advertise        :      true
       Willing          :      false
       Priority Map     :        0       0       0       1       0       0       0       0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |