Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGMP Version

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Configure the IGMP version as 3.

       SEFOS(config-if)# ip igmp version 3
       SEFOS(config-if)# end

3. Review the current IGMP router version.

       SEFOS# show ip igmp interface vlan 2

       ...
        Current IGMP router version is 3
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |