Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Boot File Name

The boot file is used by the clients to identify the boot image. In this example, the boot file name is `Image.exe`.

1. Specify the name of the boot file in use on switch 1.

       SEFOS# configure terminal
       SEFOS(config)# ip dhcp bootfile Image.exe
       SEFOS(config)# end

2. View the changes to the configuration in switch 1.

       SEFOS# show ip dhcp server information

       DHCP server status                         : Enable
       Send Ping Packets                          : Enable
       Debug level                                : None
       Server Address Reuse Timeout               : 10 secs
       Next Server Address                        : 12.0.0.5
       Boot file name                             : Image.exe

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |