Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### VLAN Administration Guide

Search Scope:

- This Document
- Entire Library

## Map a Priority to Traffic Class

You can map a priority to a traffic class on the specified port (0/2 in this example). The frame received on the interface with the configured priority is processed in the configured traffic class.

1. View the configuration information.

       SEFOS# show vlan traffic-classes port extreme-ethernet 0/2
       Traffic Class table
       ---------------------
       Port     Priority    Traffic Class
       -----    ---------   -------------
       Ex0/2    1           0
       Ex0/2    2           1
       Ex0/2    3           3
       Ex0/2    4           4
       Ex0/2    5           5
       Ex0/2    6           6
       Ex0/2    7           7

2. Map a priority to a traffic class.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/2
       SEFOS(config-if)# vlan map-priority 7 traffic-class 1
       SEFOS(config-if)# end
       SEFOS(config)# exit

3. Review the configuration information.

       SEFOS# show vlan traffic-classes port extreme-ethernet 0/2
       Traffic Class table
       ---------------------
       Port     Priority    Traffic Class
       -----    ---------   -------------
       Ex0/2    1           0
       Ex0/2    2           1
       Ex0/2    3           3
       Ex0/2    4           4
       Ex0/2    5           5
       Ex0/2    6           6
       Ex0/2    7           1

Copyright © 2010, 2011, Oracle and/or its affiliates. All rights reserved. Legal Notices |