Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Demand Circuit

This procedure enables OSPF to treat the specified interface as an OSPF demand circuit.

1. Configure `VLAN 1` as OSPF demand circuit.

       SEFOS(config-if)# ip ospf demand-circuit

2. Examine the configuration details.

       SEFOS# show ip ospf interface vlan 1

       vlan1 is line protocol is up
         Internet Address 10.4.0.1, Mask 255.255.0.0, Area 0.0.0.0
         AS 1, Router ID 10.10.2.1, Network Type BROADCAST, Cost 1
         Configured as demand circuit.
         Run as demand circuit.
         Transmit Delay is 5 sec, State 2, Priority 1
         No designated router on this network
         No backup designated router on this network
         Timer intervals configured, Hello 10, Dead 40, Wait 40, Retransmit 5
         Hello due in 4 sec
         Neighbor Count is 0, Adjacent neighbor count is 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |