Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Redistributed Route Attributes

This example configures the IPv6 address prefix as `3333::`, with a prefix length of 64. The metric value of 100 is applied to the route before it is advertised to the OSPFv3 domain, with a metric type of as Exttype1 and a tag of 10.

1. Enter the Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in SEFOS1.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.0.0.1

4. Configure the ASBR router.

       SEFOS(config-router)# asbr router

5. Configure the redistribution of static routes.

       SEFOS(config-router)# redistribute static

6. Configure the redistribution configuration.

       SEFOS(config-router)# redist-config 3333:: 64 metric-value 100 metric-type asExttype1 tag 10

7. View the effect of the configuration.

       SEFOS# show running-config ospf3

       Building configuration...
       ipv6 router ospf
       router-id 10.0.0.1
       ASBR Router
       passive-interface
       redistribute static
       redist-config 3333:: 64 metric-value 100 metric-type asExttype1 tag 10
       !
       interface vlan 11
       ipv6 ospf area 0.0.0.0
       ipv6 ospf passive-interface
       !
       interface vlan 10
       ipv6 ospf area 0.0.0.6
       ipv6 ospf passive-interface
       !

       end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |