Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable IGMP on an Individual Interface

By default, IGMP is disabled globally. You must enable IGMP globally and on the interface on which IGMP is needed.

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Enable IGMP on the interface.

       SEFOS(config-if)# set ip igmp enable
       SEFOS(config-if)# end

3. Review the configuration information.

       SEFOS# show ip igmp interface vlan 2

        vlan2, line protocol is up
        Internet Address is 12.0.0.1/8
        IGMP is enabled on interface
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |