Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

### LA Topology Example

This illustration shows the topology used in the example procedures.

By default, SEFOS supports a maximum of 8 ports per aggregation, assuming that the maximum number of ports per aggregation is 2.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |