Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable LAN Prune Delay

LAN prune delay is disabled in the system, by default.

1. Enable PIM globally.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable

2. Enter Interface Configuration mode for the interface.

       SEFOS(config)# interface vlan 5

3. Associate the VLAN interface with the PIM component.

       SEFOS(config-if)# ip pim componentId 1

4. Specify how often (in seconds) the switch sends PIM messages to the interface.

       SEFOS(config-if)# ip pim query-interval 60

5. Enable LAN prune delay.

       SEFOS# ip pim lan-prune-delay enable
       SEFOS(config-if)# end

6. Ensure the correct interval is set.

       SEFOS# show ip pim interface detail

       Vlan5 33 is up
         Internet Address is 10.1.0.1
         Muticast Switching : Enabled
         PIM : Enabled
         PIMv6 : Disabled
           PIM version : 2, mode: Sparse
           PIM DR : 10.1.0.1
           PIM DR Priority : 1
           PIM Neighbour Count : 0
           PIM Hello/Query Interval : 60
           PIM Message Interval : 60
           PIM Override Interval : 0
           PIM Lan Delay : 120
           PIM Lan-Prune-Delay : Enabled
           PIM Component Id : 1
           PIM domain border : disabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |