Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LLDP Chassis-ID Subtype

You can configure the chassis ID subtype with any of the following values:

- Chassis component

- Interface alias

- Port component

- MAC address

- Network address

- Intereface name

- Local

While configuring the chassis-ID subtype as a chassis component, port component, or local setting, you must include an input string in the command for setting the chassis ID.

1. At both switches, configure the LLDP chassis ID subtype.

       SEFOS# configure terminal
       SEFOS(config)# lldp chassis-id-subtype chassis-comp "chassis"
       SEFOS(config)# set lldp enable
       SEFOS(config)# end

2. At switch 1, review the local system information on `extreme-ethernet 0/1`.

       SEFOS# show lldp
       ...
       Chassis Id SubType            : Chassis Component
       Chassis Id                : chassis

3. At switch 2, review the detailed information of the learned, remote entry on `extreme-ethernet 0/1`.

       SEFOS# show lldp neighbors extreme-ethernet 0/1 detail
       ...
       Chassis Id SubType            : Chassis Component
       Chassis Id                : chassis
       ...

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |