Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Setting the MTU for Use in PMTU Discovery

Each PMTU value is associated with a specific path traversed by packets that are exchanged between the source and destination nodes. The PMTU value for a destination is discovered dynamically, which is the minimum PMTU of all paths through which the destination can be reached.

This procedure shows how to set the MTU for use in PMTU discovery:

- Set the MTU for Use in PMTU Discovery

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |