Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

## Configure Switch `ES1-24p-1` for L3 Routing Using RIP

1. Start the configuration with all ports and the default VLAN shutdown.

   Disable GVRP and GMRP.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# set gvrp disable
       ES1-24p-1 SEFOS(config)# set gmrp disable
       ES1-24p-1 SEFOS(config)# set port-channel enable
       ES1-24p-1 SEFOS(config)# interface vlan 1
       ES1-24p-1 SEFOS(config-if)# shutdown
       ES1-24p-1 SEFOS(config-if)# no ip address
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface range extreme-ethernet 0/1-24
       ES1-24p-1 SEFOS(config-if-range)# shutdown
       ES1-24p-1 SEFOS(config-if-range)# end

2. Create and enable port-channels between switches per the topology.

   See L2 and L3 Topology.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# interface port-channel 12
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface port-channel 13
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# end

3. Configure VLANs manually.

   You must add at least one port to the VLAN before you can assign the VLAN a name.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# vlan 2003
       ES1-24p-1 SEFOS(config-vlan)# ports add port-channel 12 untagged port-channel 12 name 192_168_203_0_RIP_P2P
       ES1-24p-1 SEFOS(config-vlan)# vlan active
       ES1-24p-1 SEFOS(config-vlan)# exit
       ES1-24p-1 SEFOS(config)# vlan 2004
       ES1-24p-1 SEFOS(config-vlan)# ports add port-channel 13 untagged port-channel 13 name 192_168_204_0_RIP_P2P
       ES1-24p-1 SEFOS(config-vlan)# vlan active
       ES1-24p-1 SEFOS(config-vlan)# exit
       ES1-24p-1 SEFOS(config)# vlan 50
       ES1-24p-1 SEFOS(config-vlan)# ports add extreme-ethernet 0/1 untagged extreme-ethernet 0/1 name 192_168_50_0_HOST_P2P
       ES1-24p-1 SEFOS(config-vlan)# vlan active
       ES1-24p-1 SEFOS(config-vlan)# exit
       ES1-24p-1 SEFOS(config)# vlan 100
       ES1-24p-1 SEFOS(config-vlan)# ports add extreme-ethernet 0/1 name access-layer-vlan-1
       ES1-24p-1 SEFOS(config-vlan)# vlan active
       ES1-24p-1 SEFOS(config-vlan)# exit
       ES1-24p-1 SEFOS(config)# vlan 101
       ES1-24p-1 SEFOS(config-vlan)# ports add extreme-ethernet 0/1 name access-layer-vlan-2
       ES1-24p-1 SEFOS(config-vlan)# vlan active
       ES1-24p-1 SEFOS(config-vlan)# end

4. Configure the port-channels as access links by setting the pvid and adding port-channels to VLANs.

   Also, disable spanning-tree on all uplinks.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# interface port-channel 12
       ES1-24p-1 SEFOS(config-if)# switchport pvid 2003
       ES1-24p-1 SEFOS(config-if)# spanning-tree disable
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface port-channel 13
       ES1-24p-1 SEFOS(config-if)# switchport pvid 2004
       ES1-24p-1 SEFOS(config-if)# spanning-tree disable
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# end

5. Add the ports to the appropriate port-channels and enable the uplink interfaces to the aggregation switches.

   Configure the host port as an access link with a different VLAN.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# interface extreme-ethernet 0/1
       ES1-24p-1 SEFOS(config-if)# description "connected to eth1 Host-1"
       ES1-24p-1 SEFOS(config-if)# switchport pvid 50
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface extreme-ethernet 0/23
       ES1-24p-1 SEFOS(config-if)# description "connected to ToR72p-1 on port67"
       ES1-24p-1 SEFOS(config-if)# channel-group 12 mode active
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface extreme-ethernet 0/21
       ES1-24p-1 SEFOS(config-if)# description "connected to ToR72p-1 on port71"
       ES1-24p-1 SEFOS(config-if)# channel-group 12 mode active
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface extreme-ethernet 0/24
       ES1-24p-1 SEFOS(config-if)# description "connected to ToR72p-2 on port68"
       ES1-24p-1 SEFOS(config-if)# channel-group 13 mode active
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface extreme-ethernet 0/22
       ES1-24p-1 SEFOS(config-if)# description "connected to ToR72p-2 on port71"
       ES1-24p-1 SEFOS(config-if)# channel-group 13 mode active
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# end

6. Configure the L3 interface for all VLANs defined previously.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# interface vlan 2003
       ES1-24p-1 SEFOS(config-if)# ip address 192.168.203.20 255.255.255.0
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 2004
       ES1-24p-1 SEFOS(config-if)# ip address 192.168.204.20 255.255.255.0
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 50
       ES1-24p-1 SEFOS(config-if)# ip address 192.168.50.10 255.255.255.0
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 100
       ES1-24p-1 SEFOS(config-if)# ip address 192.168.100.10 255.255.255.0
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 101
       ES1-24p-1 SEFOS(config-if)# ip address 192.168.101.10 255.255.255.0
       ES1-24p-1 SEFOS(config-if)# no shutdown
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# end

7. Enable RIP, and advertise the networks that are reachable through this switch.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# router rip
       ES1-24p-1 SEFOS(config-router)# version 2
       ES1-24p-1 SEFOS(config-router)# auto-summary disable
       ES1-24p-1 SEFOS(config-router)# redistribute connected
       ES1-24p-1 SEFOS(config-router)# network 192.168.203.20
       ES1-24p-1 SEFOS(config-router)# network 192.168.204.20
       ES1-24p-1 SEFOS(config-router)# network 192.168.50.10
       ES1-24p-1 SEFOS(config-router)# network 192.168.100.10
       ES1-24p-1 SEFOS(config-router)# network 192.168.101.10
       ES1-24p-1 SEFOS(config-router)# end

8. Enable the VLANs to send and receive RIP version 2 updates.

       ES1-24p-1 SEFOS# configure terminal
       ES1-24p-1 SEFOS(config)# interface vlan 2003
       ES1-24p-1 SEFOS(config-if)# ip rip send version 2
       ES1-24p-1 SEFOS(config-if)# ip rip receive version 2
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 2004
       ES1-24p-1 SEFOS(config-if)# ip rip send version 2
       ES1-24p-1 SEFOS(config-if)# ip rip receive version 2
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 50
       ES1-24p-1 SEFOS(config-if)# ip rip send version 2
       ES1-24p-1 SEFOS(config-if)# ip rip receive version 2
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 100
       ES1-24p-1 SEFOS(config-if)# ip rip send version 2
       ES1-24p-1 SEFOS(config-if)# ip rip receive version 2
       ES1-24p-1 SEFOS(config-if)# exit
       ES1-24p-1 SEFOS(config)# interface vlan 101
       ES1-24p-1 SEFOS(config-if)# ip rip send version 2
       ES1-24p-1 SEFOS(config-if)# ip rip receive version 2
       ES1-24p-1 SEFOS(config-if)# end

9. Save the configuration.

       ES1-24p-1 SEFOS# copy run start
       Building configuration ...
       [OK]
       ES1-24p-1 SEFOS#

10. Verify the status of the interfaces.

        ES1-24p-1 SEFOS# show interface description

        Interface    Status   Protocol  Description
        ---------    ------   --------  -----------
        Ex0/1        up       up        connected to eth1 Host-1
        Ex0/2        down     down
        :
        :
        Ex0/20       down     down
        Ex0/21       up       up        connected to ToR72p-1 on port71
        Ex0/22       up       up        connected to ToR72p-2 on port71
        Ex0/23       up       up        connected to ToR72p-1 on port67
        Ex0/24       up       up        connected to ToR72p-2 on port68
        po12         up       up
        po13         up       up
        vlan1        down     down
        vlan2003     up       up
        vlan2004     up       up
        vlan50       up       up
        vlan100      up       up
        vlan101      up       up

11. Verify the routes learned.

        ES1-24p-1 SEFOS# show ip route

        Codes: C - connected, S - static, R - rip, B - bgp, O - ospf

        R 192.168.9.0/24 [3] via 192.168.203.10
        R 192.168.20.0/24 [3] via 192.168.203.10
        R 192.168.30.0/24 [2] via 192.168.203.10
        R 192.168.40.0/24 [4] via 192.168.203.10
        C 192.168.50.0/24 is directly connected, vlan50
        R 192.168.60.0/24 [3] via 192.168.203.10
        C 192.168.100.0/24 is directly connected, vlan100
        C 192.168.101.0/24 is directly connected, vlan101
        R 192.168.150.0/24 [3] via 192.168.203.10
        R 192.168.151.0/24 [3] via 192.168.203.10
        R 192.168.201.0/24 [2] via 192.168.203.10
        R 192.168.202.0/24 [3] via 192.168.203.10
        C 192.168.203.0/24 is directly connected, vlan2003
        C 192.168.204.0/24 is directly connected, vlan2004
        R 192.168.205.0/24 [2] via 192.168.203.10
        R 192.168.206.0/24 [3] via 192.168.203.10
        R 45.45.45.0/24 [3] via 192.168.203.10
        R 45.45.46.0/24 [3] via 192.168.203.10
        R 45.45.47.0/24 [3] via 192.168.203.10
        R 45.45.48.0/24 [3] via 192.168.203.10
        R 45.45.49.0/24 [3] via 192.168.203.10
        R 45.45.50.0/24 [3] via 192.168.203.10
        R 45.45.51.0/24 [3] via 192.168.203.10
        ...

12. Verify the number of routes.

    After IXIA sends 500 routes to the core switch, those routes are learned on this switch.

        ES1-24p-1 SEFOS# show ip route summary

        Route Source    Routes
        connected         5
        static            0
        rip               511
        bgp               0
        ospf              0
        Total             516

##### Related Information

- Configure Switch `TOR72p-1` for L3 Routing Using RIP

- Configure Switch `TOR72p-2` for L3 Routing Using RIP

- Configure Switch `ES1-24p-2` for L3 Routing Using RIP

- Verify the L3 RIP Configuration

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |