Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Stub Area, ASBR, and Route Redistribution

You can configure area parameters only after enabling the OSPF process. You configure area parameters in Router Configuration mode.

- Stub Area, ASBR, and Route Redistribution Topology Example

- Configure the Stub Area

- Configure the ASBR Router

- Disable the ASBR Router

- Configure Redistribution

- Disable Redistribution of Routes

- Configure SEFOS4

- Configure SEFOS5

- Configure SEFOS7

- Examine the Configuration Details in SEFOS4

- Examine the Redistributed External Routes in SEFOS5

- Examine the External Routes Not Distributed in Stub Area `0.0.0.4` in SEFOS7

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |