Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Overflow Exit Interval

Configuring the overflow exit interval specifies how much time must pass (in seconds) before a router will attempt to leave the overflow state. If you specify a value of 0, the router will remain in the overflow state.

- Configure the Overflow Exit Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |