Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring a Multicast Router Port

You can configure multicast router ports for a VLAN statically, or the port can be learned dynamically. Whenever a port receives a query message, then that port is also added to the multicast router port list. This section contains procedures that explain how to enable or disable multicast router ports. Before you can configure IGS features, you must configure your network environment, as described in Topology Example.

- Enable Multicast Router Port

- Disable a Multicast Router Port

- Configure the Multicast Router Port Time-Out Value

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |