Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Port-Purge Interval

When the port purge timer on a port for a particular multicast group expires, the port is removed from the forwarding list of the corresponding multicast entry in the multicast forwarding table.

- Configure the Port-Purge Interval

- Restore the Port-Purge Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |