Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LACP System Identifier

In the following procedure, ports 0/1, 0/2, and 0/3 are part of the LA. Unless otherwise noted, you must run all of the commands in the following procedure on both switches.

1. Enable port channeling.

       SEFOS# configure terminal
       SEFOS(config)# set port-channel enable

2. Create the port channel (1 in this example).

       SEFOS(config)# interface port-channel 1
       SEFOS(config-if)# no shutdown
       SEFOS(config)# end

3. Configure the LACP system identifier.

       SEFOS(config)# lacp system-identifier 00:55:44:33:22:11
       SEFOS(config)# end

4. Review the `etherchannel` information to ensure that the port channel system identifier has been set.

   The output has been truncated for readability.

       SEFOS# show etherchannel detail

       ...
       Port-channel System Identifier is  00:55:44:33:22:11
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |