Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Connect the NET MGT Cable

1. Install the switch in the rack

   See Install the Switch in the Rack.

2. Connect the network management cable from the management console to the connector labeled NET MGT 0 (Port A).

   See NET MGT Port.

   Note - Use NET MGT 0 (Port A) only. Do not use NET MGT 1 (Port B). Port B is functional but currently has some limitations and is not supported at this time.

3. Configure the DHCP server with the MAC address of the management controller.

   The MAC address is printed on the (yellow) customer information sheet on the outside of the switch shipping carton.

4. Route the management cables so that they do not interfere with other cables, with servicing the switch, or with other systems.
5. Prepare the management console for communication with the management controller.
6. Power on the switch.

   See Power On the Switch.

##### Related Information

- NET MGT Port

- Management Cable Requirements

- Connect Ethernet Cables

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |