Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Remove a Fan

Note - Fans are hot-swappable and do not require powering off.

| Caution - The switch can continue to run safely with one failed fan. If a fan fails, replace it as soon as possible. The system might overheat if more than one fan fails.

1. Determine which fan is to be removed.

   If a fan has failed, its Attention LED lights.

2. Loosen the captive thumbscrew at the right side of the fan.
3. Grasp the handle and pull the fan straight out.
4. Set the fan aside.
5. Consider your next step:
   - If you are removing the fan for replacement, install a new fan.

     See Install a Fan.

   - If you are removing the fan as a subtractive action, you are finished.

##### Related Information

- Remove a Power Supply

- Install a Fan

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |