Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGS Version

You can configure the operating version of the IGS switch for a specific VLAN as v1, v2, or v3. By default, the operating version of the IGS switch for all of the VLANs is v3. Before you can configure IGS features, you must already configure your network environment, as described in Topology Example.

1. Enter the configure mode for the VLAN interface.

       SEFOS# configure terminal
       SEFOS(config)# vlan 4

2. Configure the IGS version.

       SEFOS(config-vlan)# ip igmp snooping version v2
       SEFOS(config)# end

3. Review the configuration.

       SEFOS# show ip igmp snooping vlan 4

       Snooping VLAN Configuration for the VLAN 4
         IGMP Snooping enabled
         IGMP configured version is V2
         Fast leave is disabled
         Snooping switch is acting as Non-Querier
         Query interval is 125 seconds

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |