Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Forward MLD Reports Only to Router Ports

If you have previously configured MLD reports to forward to all ports, you can restore the default setting to forward MLD reports to only router ports on a VLAN.

1. Reconfigure the forwarding of reports to only router ports.

       SEFOS# configure terminal
       SEFOS(config)# ipv6 mld snooping report-forward router-ports
       SEFOS(config)# end

2. View the configuration.

       SEFOS# show ipv6 mld snooping globals

       Snooping Configuration
       -----------------------------
       MLD Snooping globally enabled
       MLD Snooping is operationally enabled
       Multicast forwarding mode is MAC based
       Proxy reporting globally enabled
       Router port purge interval is 125 seconds
       Port purge interval is 130 seconds
       Report forward interval is 8 seconds
       Group specific query interval is 3 seconds
       Reports are forwarded on router ports
       Group specific query retry count is 4

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |