Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

## Configuring L3 Routing Based Topology Using RIP

These tasks describe how to configure each switch to learn routes through L3 RIP.

- Configure Switch `TOR72p-1` for L3 Routing Using RIP

- Configure Switch `TOR72p-2` for L3 Routing Using RIP

- Configure Switch `ES1-24p-1` for L3 Routing Using RIP

- Configure Switch `ES1-24p-2` for L3 Routing Using RIP

- Verify the L3 RIP Configuration

##### Related Information

- Switches Overview

- Understanding L2 and L3 Implementations

- L2 Based Configuration Example Using PVRST Protocol

- Configuring a Basic L2 PVRST Based Topology

- Configuring an L2 PVRST Based Topology With Active/Standby Bond on the Servers

- Configuring an L2 PVRST and LLA Based Topology With Active/Active Bond on the Servers

- L3 RIP and OSPF Configuration Overview

- Configuring L3 Routing Based Topology Using OSPF

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |