Using This Documentation

This manual provides SEFOS CLI Enterprise command descriptions, syntax, and examples for the Sun Network 10GbE Switch 72p and Sun Blade 6000 Ethernet Switched NEM 24p 10GbE. You are expected to have a basic knowledge of Ethernet switching and routing administration as a prerequisite to using this manual. SEFOS is accessed through Oracle ILOM. For instructions on connecting to Oracle ILOM and SEFOS, refer to the user’s guide for your switch.

- Product Notes

- Related Documentation

- Acronyms and Abbreviations

- CLI Command Modes

- Feedback

- Support and Accessibility

##

Product Notes

For late-breaking information and known issues about the following products, refer to the product notes at:

Sun Blade 6000 Ethernet Switched NEM 24p 10GbE:

`http://www.oracle.com/pls/topic/lookup?ctx=SB6K-24p-10GbE`

Sun Network 10GbE Switch 72p:

`http://www.oracle.com/pls/topic/lookup?ctx=SN-10GbE-72p`

##

Related Documentation

Documentation | Links
--- | ---
All Oracle products | `http://oracle.com/documentation`
Sun Blade 6000 Ethernet Switched NEM 24p 10GbE | `http://www.oracle.com/pls/topic/lookup?ctx=SB6K-24p-10GbE`
Sun Network 10GbE Switch 72p | `http://www.oracle.com/pls/topic/lookup?ctx=SN-10GbE-72p`
Sun Blade 6000 modular system | `http://www.oracle.com/pls/topic/lookup?ctx=sb6000`
Oracle Integrated Lights Out Manager (Oracle ILOM) 3.0 | `http://www.oracle.com/pls/topic/lookup?ctx=ilom30`

Table providing related documentation URLs.

For detailed information about the commands and options described in this document, refer to the Sun Ethernet Fabric Operating System CLI Base Reference Manual.

##

Acronyms and Abbreviations

The following acronyms and abbreviations are used in this book:

Acronym or Abbreviation | Explanation
--- | ---
AARP | AppleTalk Address Resolution
ACL | Access control list
APNIC | Asia-Pacific Network Information Centre
ARIN | American Registry for Internet Addresses
ARP | Address Resolution Protocol
AS | Autonomous system
ASBR | Autonomous border system router
BGP | Border Gateway Protocol
BPBDU | Bridge protocol data unit
BSD | Berkeley Software Distribution
CBS | Committed burst size
CEP | Customer edge port
CIDR | Classless inter-domain routing
CIR | Committed information rate
CIST | Common Internal Spanning Tree
CMM | Chassis Management Module
CNA | Converged netwaork adapter
DCB | Data cebter bridging
DCBX | Data Center Exchange Protocol
DEC | Digital Equipment Corporation
DSCP | Differentiated services code point
EBS | Excess burst size
EF DSCP | Expidited forwarding DSCP
EIR | Excess information rate
ETS | Enhancement transmission selection
EIGRP | Enhanced Interior Gateway Protocol
FCoE | Fiber Channel over Ethernet
FDB | Forwarding database
FSAP | Flexible software architecture for portability
GARP | Generic Attribute Registration Protocol
GMRP | GARP Multicast Registration Protocol
GVRP | GARP VLAN Registration Protocol
ICMP | Internet Control Message Protocol
ICMPv4 | Internet Control Message Protocol version 4
IGMP | Internet Group Management Protocol
IGS | IGMP snooping
IP TOS | IP type of service
ISL | Inter-switch link
IVL | Independent VLAN learning
LA | Link aggregation
LACP | Link aggregation Control Protocol
LACNIC | Latin American and Caribbean Network Information Centre
LLDP | Link Layer Discovery Protocol
MEF | Metro Ethernet Forum
MIB | Management information base
MLD | Multicast listener discovery
MLDS | Multicast listener discovery snooping
MSTP | Multiple Spanning Tree Protocol
NetBIOS | Network Basic Input/Output System
NPAPI | Network processor application programming interface
OPSF | Open Shortest Path First
PDU | Protocol description unit
PFC | Priority-based flow control
PG | Priority group
PHB | Per-hop behavior
PIM | Protocol independent multicast
PMTU | Path MTU
PMTUD | PMTU discovery
PVID | Port VLANI ID
PVRST | Per-VLAN Rapid Spanning Tree
PVRST+ | Per-VLAN Rapid Spanning Tree Plus
PVST | Per-VLAN Spanning Tree
RFC | Request for comments
RIP | Routing Information Protocol
RIPE NCC | Reseaux IP Europeens Network Coordination Centre
RMON | Remote monitoring
RRD | Route redistribution
RST | Rapid Spanning Tree
RTM | Route table manager
SLA | service-level agreement
SLI | Socket layer interface
SNMP | Simple Network Management Protocol
srTCM | Single rate three color marker
STP | Spanning Tree Protocol
SVL | Shared VLAN learning
TCP/IP | Transmission Control Protocol/Internet Protocol
TCP ACK bit | TCP acknowledgement bit
TCP RST bit | TCP reset bit
TCN | Topology change notification
TFTP | Trivial File Transfer Protocol
trTCM | Two rate three color marker
TSWTCM | Time sliding window three color marker
TLV | Type, length, and value
TTL | Time-to-live value
UDP | User Datagram Protocol
VINES | Virtual integrated network service
VLAN | Virtual LAN
VLAN ID | VLAN identifier
XNS | Xerox network systems
XVLAN | Exclusive VLAN

Table defining the acronyms and abbreviations used in this document.

##

CLI Command Modes

The following table provides the access and exit methods to various general configuration modes.The following table lists the different CLI command modes.

Command Mode | Access Method | Prompt | Exit Method
--- | --- | --- | ---
User EXEC | Initial mode to start a session. | `SEFOS>` | Use the logout method.
Privileged EXEC | Use the `enable` command from User EXEC mode. | `SEFOS#` | Use the `disable` command to return to User EXEC mode.
Global Configuration | Use the `configure terminal` command from Privileged EXEC mode. | `SEFOS(config)#` | Use the `end` command to return to Privileged EXEC mode.
Interface Configuration | Use the `interface` interface-type interface-id from Global Configuration mode command. | `SEFOS(config-if)#` | Use the `exit` command to return to Global Configuration mode
Interface Range Configuration | Use the `interface range` command from Global Configuration mode. | SEFOS(config-if-range)# | Use the `exit` command to return to Global Configuration mode.
Config-VLAN | Use the `vlan vlan-id` command from Global Configuration mode. | SEFOS(config-vlan)# | Use the `exit` command to return to Global Configuration mode.
Line Configuration | Use the `line` command from Global Configuration mode. | SEFOS(config-line)# | Use the `exit` command to return to Global Configuration mode.
Profile Configuration | Use the `ip mcast profile` profile-id`[description (128)]` from Global Configuration mode. | SEFOS(config-profile)# | Use the `exit` command to return to Global Configuration mode.

Table describing the CLI command modes used in this document.

##

Feedback

Provide feedback on this documentation at:

`http://www.oracle.com/goto/docfeedback`

##

Support and Accessibility

Description | Links
--- | ---
Access electronic support through My Oracle Support | `http://support.oracle.com` For hearing impaired: `http://www.oracle.com/accessibility/support.html`
Learn about Oracle’s commitment to accessibility | `http://www.oracle.com/us/corporate/accessibility/index.html`

Table listing the support and accessibility URLs.

Copyright © 2012, Oracle and/or its affiliates. All rights reserved.