Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default Value of the OSPF Transmission Delay

The default time for transmitting a link state update packet on an interface is 1 second.

- Type.

      SEFOS(config-if)# no ip ospf transmit-delay

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |