Go to main content
oracle home
Sun Network 10GbE Switch 72p Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: November 2016

- Sun Network 10GbE Switch 72p Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Late-Breaking Information

- Switch Documentation Reading Order
- New Features

- IPv6 Switching and Routing
- PVRST+ Protocol
- Exclusive VLAN
- Data Center Bridging
- Internet Group Management Protocol
- PIM
- Q-in-Q Tunneling
- Server Load Balancer Layer 3
- Uplink Port Trailing
- VRRPv3
- Oracle ILOM 3.0 Features

- Enhancements
- Upgrading the Switch Firmware

- Back Up the Current Configuration Before Upgrading
- Download the Switch Firmware Package
- Install the Switch Updates

- Configuring the Switch

- Configure 1Gbps Mode on SFP+ Interfaces
- Fine Tune the VLAN Setup
- Managing SEFOS Configurations

- Include the SEFOS Configuration in Backups
- Restore the Configuration

- Configuring TACACS+

- TACACS+ Properties
- Configure TACACS+ Settings

- Known Issues

- Manually Deleting Static Routes Does Not Affect the Corresponding SLB Entry (7123134)
- PIMv6-SSM Mode is Not Supported in This Release (7114280)
- Firmware Upgrade With the Web UI is Incomplete (7022295)
- Changing the Default Value for default-vlan-id Could Result in VLAN Misconfiguration (7015004)
- Some of the IGMP Conformance Results Do Not Match Expectations (7006297 and 6997415)
- QoS - set algo-type tailDrop queue-drop-algo Does Not Work (6991230)
- Packets Might Be Dropped When Using Q-in-Q Interop in Certain Configurations (6989048)
- The no default-metric [,short(1-16)>] Command Does Not Work as Documented (6987482)
- Using vlan 1 as Shown in Various Examples in the Documentation Generates Error Codes (6968484)
- When Multiple Configuration Scripts Are Run in Parallel, SEFOS Can Crash (6936742)
- The switch Command Line Option Is Unsupported
- vrrp_v3: Role is incorrect for vlan with no premempt configuration after save/reboot (19547263)
- SSL V3.0 POODLE DISABLE SSL V3 (19842635)
- Re-configure IP address after a "no ip address", previous config re-appears (18794861)

Language:

### Exclusive VLAN

In a traditional VLAN, the VLAN represents an L3 broadcast domain or a subnet. Exclusive VLAN (XVLAN) provides a discrete isolation of ports belonging to a traditional VLAN. Therefore, one host in an XVLAN can communicate with some of the hosts in the XVLAN, while another host cannot do the same even though they are in the same XVLAN and configured in the same subnet.

Refer to the Sun Ethernet Fabric Operating System XVLAN Administration Guide for more information about this feature. For information about supported XVLAN commands, refer to the Sun Ethernet Fabric Operating System CLI Base Reference Manual.

Note - See Changing the Default Value for default-vlan-id Could Result in VLAN Misconfiguration (7015004) for information about the required settings for default-vlan-id in XVLAN configurations.

Previous
Next