Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure an Internal Address Range

This example configures an internal address range in SEFOS1.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in SEFOS1.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.0.0.1

4. Configure the entire summary for this `fec0::1111:0:0` address range.

       SEFOS(config-router)# area 0.0.0.6 range fec0::1111:0:0 96 advertise summary

5. View the results in SEFOS1.

       SEFOS# show ipv6 ospf area 0.0.0.0 database  detail

       Age: 0   Seconds            LS Type: Link Lsa
       Link State Id: 0.0.0.41     Adv Rtr Id: 10.0.0.1
       Sequence: 0x8000001f        Checksum: 0xc50c    Length: 60
       Router Priority: 1          Options: 0x33
       Prefix: fe80::214:4fff:fe6c:628f
       #Prefixes: 1
       Prefix Length (Bytes): 12   Prefix Options: 0x00
       Prefix: fec0::2856:0:0
       Age: 3   Seconds            LS Type: Link Lsa
       Link State Id: 0.0.0.40     Adv Rtr Id: 10.0.0.8
       Sequence: 0x8000001f        Checksum: 0xda3b    Length: 60
       Router Priority: 1          Options: 0x33
       Prefix: fe80::221:28ff:fe54:7069
       #Prefixes: 1
       Prefix Length (Bytes): 12   Prefix Options: 0x00
       Prefix: fec0::2856:0:0

       Age: 0   Seconds            LS Type: Router Lsa
       Link State Id: 0.0.0.0      Adv Rtr Id: 10.0.0.1
       Sequence: 0x80000020        Checksum: 0x0e62    Length: 40
       Router is an Area Border Router
       Number of Links: 1          Options: 0x33
       Link connected to : transit network
       Metric: 0x1                 Interface Id: 41
       Nbr Interface Id: 40        Nbr Router Id: 10.0.0.8

       Age: 3   Seconds            LS Type: Router Lsa
       Link State Id: 0.0.0.0      Adv Rtr Id: 10.0.0.8
       Sequence: 0x80000020        Checksum: 0xd890    Length: 40
       Router is an AS Boundary Router
       Number of Links: 1          Options: 0x33
       Link connected to : transit network
       Metric: 0x1                 Interface Id: 40
       Nbr Interface Id: 40        Nbr Router Id: 10.0.0.8

       Age: 3   Seconds            LS Type: Network Lsa
       Link State Id: 0.0.0.40     Adv Rtr Id: 10.0.0.8
       Sequence: 0x8000001f        Checksum: 0xabe7    Length: 32
       Options: 0x33
       Attached Router: 10.0.0.8
       Attached Router: 10.0.0.1
       Age: 3   Seconds            LS Type: Intra Area Prefix Lsa
       Link State Id: 0.0.0.0      Adv Rtr Id: 10.0.0.8
       Sequence: 0x80000040        Checksum: 0xdff7    Length: 48
       #Prefixes: 1                Referenced LS Type: Network Lsa
       Ref Link State Id: 0.0.0.40  Ref Adv Router: 10.0.0.8
       Prefix Length (Bytes): 12    Prefix Options: 0x00
       Metric: 0x0
       Prefix: fec0::2856:0:0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |