Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### QoS Administration Guide

Search Scope:

- This Document
- Entire Library

### Introduction

Configuring QoS on a Sun Blade 6000 Ethernet Switched NEM 24p 10GbE or switch involves the following three steps:

1. Classifying and conditioning the ingress traffic of interest.

2. Configuring the egress port queuing and scheduling.

3. Mapping the ingress traffic to egress queues.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |