Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

#### Default MSTP Settings

By default, only one spanning tree is running on the bridge. For other default configurations of MSTP, see Default MSTP Settings.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |