Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the RIP Packet Retransmission Interval and Retry Count

Before you can configure the retransmission level or retry count, you must configure your environment. The procedures in this section are based on RIP Topology 1. For instructions on how to configure switch 1, see Configure Switch 1. For instructions on how to configure switch 2, see Configure Switch 2.

- Set the RIP Packet Retransmission Interval and Retry Count

- Reset the Retransmission Interval and Retry Count

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |