Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Debugging

- Enable the debug level.

      SEFOS 1 SEFOS# debug ipv6 rip all

      RIP6: RIP6 : Got a update timer expiry on If = 41
      RIP6: RIP6: Send RIP6 resp Dest port = 521 If = 41 Resp flag = 1 Dest Addr = ff02::9
      RIP6: RIP6BUF: In bufwrite Bufptr = 0x11277798 data = 0x3cb9340e offset = 0 size = 4 Copy = 1
      RIP6: RIP6:Combining routes over If=41 RespFlag=1 Horizon=1 DestPort=521 DestAddr=ff02::9
      RIP6: Sending over If=41 Route counter=0 Max no of RTE= 456 Len=4 BufPtr=0x3cb932f0
      RIP6: RIP6BUF: In bufwrite Bufptr = 0x11277798 data = 0x3cb93280 offset = 4 size = 20 Copy = 1
      RIP6: RIP6:Combining routes over If=41 RespFlag=1 Horizon=1 DestPort=521 DestAddr=ff02::9
      RIP6: Sending over If=41 Route counter=1 Max no of RTE= 456 Len=24 BufPtr=0x3cb932f0
      RIP6: RIP6BUF: In bufwrite Bufptr = 0x11277798 data = 0x3cb93280 offset = 24 size = 20 Copy = 1
      RIP6: RIP6:Combining routes over If=41 RespFlag=1 Horizon=1 DestPort=521 DestAddr=ff02::9
      RIP6: Sending over If=41 Route counter=2 Max no of RTE= 456 Len=44 BufPtr=0x3cb932f0
      RIP6: RIP6BUF: In bufwrite Bufptr = 0x11277798 data = 0x3cb93280 offset = 44 size = 20 Copy = 1
      RIP6: RIP6:Combining routes over If=41 RespFlag=1 Horizon=1 DestPort=521 DestAddr=ff02::9
      RIP6: Sending over If=41 Route counter=3 Max no of RTE= 456 Len=64 BufPtr=0x3cb932f0
      RIP6: RIP6BUF: In bufwrite Bufptr = 0x11277798 data = 0x3cb93280 offset = 64 size = 20 Copy = 1
      RIP6: RIP6:Combining routes over If=41 RespFlag=1 Horizon=1 DestPort=521 DestAddr=ff02::9
      RIP6: Sending over If=41 Route counter=4 Max no of RTE= 456 Len=84 BufPtr=0x3cb932f0
      RIP6: RIP6BUF: In bufwrite Bufptr = 0x11277798 data = 0x3cb93280 offset = 84 size = 20 Copy = 1
      RIP6: RIP6:Combining routes over If=41 RespFlag=1 Horizon=1 DestPort=521 DestAddr=ff02::9
      RIP6: Sending over If=41 Route counter=5 Max no of RTE= 456 Len=104 BufPtr=0x3cb932f0
      RIP6: RIP6BUF: In bufwrite Bufptr = 0x11277798 data = 0x3cb93280 offset = 104 size = 20 Copy = 1
      RIP6: RIP6:RIP6 send Buf=0x11277798 Send flag=1 DstUDP6Port=521 If=41 DestAddr=ff02::9 Len=124
      RIP6: RIP6LIB: Starting timer Id = 3 Duration = 30 Timer Node = 0x11702424
      RIP6: RIP6BUF: Reading from buf = 0x112777f8 data = 0x3cb934f4 offset = 0 size = 4 copy = 0
      RIP6: RIP6BUF: Returning pointer = 0x35840d80 local data = 0x3cb934f4
      RIP6: RIP6 : The RIP6 header has Command = 2 Version = 1 Reserved field = 0
      RIP6: RIP6:rcvd resp Buf=0x112777f8 HopLim=255 Len=124 If=41 SrcAddr=ff02::9 DestAddr=fe80::221:28ff:fe56:d7a9
      RIP6: RIP6 : Received RIP6 response buffer :
      RIP6: RIP6:sndrOfRIPngRespDidnt putLlocalSrcAddr RespCameOnIf=41 SrcAddr=FF02:0000:0000:0000:0000:0000:0000:0009 DesAddr=FE80:0000:0000:0000:0221:28FF

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |